**Appendix – I**

**(Schedule of Quantity)**

|  |  |  |
| --- | --- | --- |
| **Sr. No.** | **Name of Item/Equipment** | **Qty.** |
| 1 | **Digital Storage Oscilloscope -2 Channel**  **Possible Company / Make**: Keysight / Tektronix / Aplab / Agilent   * Digital Oscilloscope, 2 Channel, 200 MHz, 2 GSPS, 1 Mpts, 1.75 ns * High resolution 8.5-inch WVGA (800 x 480) display * Up to 200,000 wfms/s update rate * Fast, responsive MegaZoom IV deep memory, 1Mpts and segmented memory * WaveGen built-in function generator (optional) * Upgradable bandwidth, MSO, WaveGen built-in 20MHz function generator and measurement applications * Connectivity: USB host (one front, one back), USB device, LAN (optional), GPIB (optional) * Connectivity: USB host (one front, one back), USB device, LAN (optional), GPIB (optional) | 02 |