**Appendix - II**

**(Schedule of Quantity)**

|  |  |  |
| --- | --- | --- |
| **Sr. No.** | **Name of Item/Equipment** | **Qty.** |
| 2 | **Digital Storage Oscilloscope - 4 Channel**  **Possible Company / Make:** Keysight / Tektronix / Aplab / Agilent   * Digital Oscilloscope, 4 Channel, minimum 100 MHz, 4 GSPS, 2 Mpts, 3.5 ns * 100 MHz Bandwidth, 2 GSa/s sample rate, 2 Mpts memory depth and a 21,6 cm TFT Display (8,5 Zoll). Upgradable to a MSO with a 8 channel logic analyzer, 1 channel 20 MHz waveform generator. * High resolution 8.5-inch WVGA (800 x 480) display * Up to 1,000,000 wfms/s update rate * Fast, responsive MegaZoom IV deep memory, up to 4M * Serial protocol analyser (optional) * Upgradable bandwidth, memory, MSO, WaveGen built-in 20MHz function generator and measurement apps * Connectivity: USB host (one front, one back), USB device, LAN (optional), GPIB (optional) | 03 |