**Appendix – IX**

**(Schedule of Quantity)**

|  |  |  |
| --- | --- | --- |
| **Sr. No.** | **Name of Item/Equipment** | **Qty.** |
| 9 | **DSP Fixed Point Statater Kits with Code Composer Studio (CCS)**   * Four 3.5mm audio jacks for microphone, line in, speaker and line out * 512K words of Flash and 16 MB SDRAM * Expansion port connector for plug-in modules * On-board standard IEEE JTAG interface * +5V universal power supply * A complete Integrated Development Environment (IDE), an efficient optimizing C/C++ compiler assembler, linker, debugger, an a advanced editor with Code Maestro™ project manager * "Plug-in" ability for third-party software for additional functionality * C6713 DSP Development Board with 512K Flash and 16MB SDRAM * C6713 DSK Code Composer Studio™ IDE including the Fast Simulators and access to Analysis Toolkit on Update Advisor | 02 |